Installation Guide for 160M Module Wall‑mount Bracket

1、Mount the main body of the wall‑mount bracket onto the wall using stainless steel screws A36021219, M8×20, 6 pcs.
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2、Mount the top hanging plate, using stainless steel screws A36021219, M8×20, 4 pcs.
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3、Mount the bottom connection plate with stainless steel screws A36021218, M6×16, 4 pcs.
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4、Hang the module onto the main wall‑mount bracket, align the holes, and fasten with stainless steel screws A36021219, M8×20, 4 pcs.
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